STANDARD DEPARTURE CHART INSTRUMENT – (SID)

DEPARTURE PROCEDURE TUCAN RWY 28

INITIAL CLIMB

Climb on TIK R-282 to cross D8 TIK at or above 2000’, then turn left 160° heading climbing to at or above 10000’ to intercept TIK R-194 in accordance with ATC instructions.

This SID requires a minimum climb gradient of 300’ per NM.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| INITIAL CLIMB  Climb on TIK R-282 to cross D8 TIK at or above 2000 ft, then turn left 160° heading climbing to at or above 10000 ft to intercept TIK R-194 in accordance with ATC instructions. | | | | | | |
| This SID requires a minimum climb gradient of 300’ per NM. | | | | | | |
| GND speed-KT | 75 | 100 | 150 | 200 | 250 | 300 |
| 300’ per NM | 375 | 500 | 750 | 1000 | 1250 | 1500 |