STANDARD DEPARTURE CHART INSTRUMENT – (SID)

DEPARTURE PROCEDURE BENIT RWY 28

Trans ALT: 19000’ Trans LEVEL: FL200

INITIAL CLIMB

Climb on runway heading.

TRANSITIONS

|  |  |
| --- | --- |
| Trans ALT: 19000’ Trans LEVEL: FL200 | |
| INITIAL CLIMB: Climb on runway heading. | |
| TRANSITIONS | |
| DEPARTURE | ROUTING |
| ALIGO | Reaching 1500 ft or above, turn right on 080° heading to intercept B-518, cross ALIGO at 4000 ft or above, then according to ATC instructions. |
| AMARU | Reaching 1500 ft or above, turn right on 060° heading to intercept G-757, cross AMARU at 4000 ft or above, then according to ATC instructions. |
| EMEMA | Reaching 1500 ft or above, turn right on 010° heading to intercept H-1, cross EMEMA at 4000 ft or above, then according to ATC instructions. |