|  |  |
| --- | --- |
| **CVA SEGMENT OUTBOUND ONLY**  AVAILABLE ALTITUDES 065, 075, 085, 095 AND 105 LEAVING MIRAM FIX, CONTINÚE WITH ALTITUDE IN ACCORDANCE WITH YOUR COURSE, NOTIFY ATC. | **GENERAL INSTRUCTIONS:**  INTERNATIONAL AIRPORT TOBIAS BOLAÑOS RWY 09 IN USE.  **OUTBOUND SEGMENT (ONLY FOR AIRCRAFT CAT A/B):**  START TURNING LEFT AT 4 000FT OVER MEXICO HOSPITAL, CONTINUE CLIMBING TO 4 500FT DO NOT EXCEED MACDO FIX, THEN TO AMAZO ON HDG 290°, TURN LEFT ON HDG 263° TO SANAT FIX, WAIT FOR UPPER LEVEL ACCORDING TO ATC INSTRUCTIONS, IF REQUIRED AT 118.6 MHZ.  **INBOUND SEGMENT**  LEAVE SANAT FIX TO ENTER AIR TRAFFIC CIRCUIT AND WAIT ATC INSTRUCTIONS. |
| **CVB SEGMENT INBOUND ONLY**  ENTERING OVER FIX SALVA CROSS AT 9 500FT MAXIMUM ALTITUDE. ALTITUDE AVAILABLES 065, 075, 085, 095 FT AWAITING INSTRUCTIONS FROM ATC. |
| **CVC SEGMENT INBOUND – OUTBOUND**  AVAILABLE ALTITUDES 045, 055 AND 065 LEAVING CASCA FIX CONTINUE WITH ALTITUDE ACCORDING YOUR COURSE, NOTIFY ATC. |